Lx 1

3

1

6

2

12

12

7

9

4

5

7

4

8

Lx 4

Lx 3

Lx 2

5 floor-based practicals. 3 are 15 amp to be patched in. 2 are 13 amp controlled by the actor

Music either on CD or from company laptop

Distance between bar 1 and setting line should be at least 5 mt.

We use a smoke machine

We need and operator for sound and lights

1. 1K FRESNEL, BACK LIGHT, GEL 161
2. PROFILE ON MEGAPHONE, 201 small
3. PROFILE ON POT, 201 small
4. 1K FRESNEL OR FLOOD, 119
5. PROFILE, 201 small
6. PROFILE, 201
7. PROFILE, 201
8. PROFILE, 201 small
9. 1K FRESNEL, BACK LIGHT, 201
10. PROFILE, 201
11. PROFILE O/W
12. 1K FRESNEL O/W
13. PROFILE, 201 small
14. PROFILE, 201 small

14

7

9

10

9

9

SETTING LINE

11

12

12

13

4

4

7

1

1

1